{"text_format":"3","workbook":"xlsx","n_sheets":10,"sheets":["净水处理间","汽车修理间","综合楼","生活蓄水池","设备用房","污水处理间","蓄水池","室外工程","充电桩车棚光伏","充电桩"],"read":"whole","date_system":"1900"}

{"sheet":"净水处理间","index":0,"n_rows":51,"n_cols":7,"rows_kept":51,"merged":[[0,0,0,5]]}
["S10尖山服务区材料统计"]
["编号","材料名称","规格型号","数量","单位","备注","单价/元"]
[1.1,"复合土工膜","质量≥600g/m2，膜材厚度≥0.3mm，CBR顶坡强度≥3.0KN，耐静水压≥0.6MPa",1,"㎡"]
[1.2,"混凝土","C20",1,"m3"]
[1.3,"混凝土","C40",1,"m3"]
[1.4,"加气混凝土块","300mm",1,"m3"]
[1.5,"炉渣",null,1,"m3"]
[1.6,"混凝土","C35",1,"m3"]
[1.7,"混凝土","C30",1,"m3"]
[1.8,"钢筋","HRB400，Φ6.5-10",1,"t"]
[1.9,"钢筋","HRB400，Φ12-14",1,"t"]
[2,"钢筋","HRB400，Φ16-25",1,"t"]
[2.1,"钢筋机械连接","直螺纹连接，钢筋直径:25mm以内",1,"个"]
[2.2,"屋面卷材防水","4mm厚SBS防水层",1,"㎡"]
[2.3,"PVC管","DN100",1,"米"]
[2.4,"岩棉板","40厚岩棉板",1,"㎡"]
[2.5,"乳胶漆","内墙面漆",1,"㎡"]
[2.6,"氟碳漆",null,1,"㎡"]
[2.7,"钢质保温防盗防火门","1800*2400",1,"樘"]
[2.8,"金属（塑钢、断桥）窗","2100*1800",1,"樘"]
[2.9,"金属（塑钢、断桥）窗","3000*1600",1,"樘"]
[3,"窗台板",null,1,"㎡"]
[1.1,"等电位箱",null,1,"台"]
[1.2,"配电箱","照明总配电箱",1,"台"]
[1.3,"控制箱","与设备配套",1,"台"]
[1.4,"防尘防水灯","30W",1,"套"]
[1.5,"密闭三级照明开关","10A 250V",1,"台"]
[1.6,"电力电缆","YJV-1KV-4*25+1*16",1,"米"]
[1.7,"电力电缆","YJV-1KV-4*35+1*16",1,"米"]
[1.8,"电力电缆","YJV-1KV-5*4",1,"米"]
[1.9,"电力电缆","YJV-1KV-5*10",1,"米"]
[2,"电力电线","RVVP4*1.5",1,"米"]
[2.1,"电力电线","BV-2.5",1,"米"]
[2.2,"PVC管","DN20",1,"米"]
[2.3,"PVC管","DN25",1,"米"]
[2.4,"PVC管","DN40",1,"米"]
[2.5,"PVC管","DN50",1,"米"]
[2.6,"镀锌钢管","Φ50mm",1,"米"]
[2.7,"镀锌扁钢","-40mm",1,"米"]
[2.8,"镀锌圆钢","Φ12mm",1,"米"]
[1.1,"热镀锌钢管","DN25",1,"米"]
[1.2,"热镀锌钢管","DN32",1,"米"]
[1.3,"柔性泡沫橡胶","厚35mm、Φ32mm",1,"㎡"]
[1.4,"管道支架","L50角钢",1,"kg"]
[1.5,"两通锁闭温控调节阀","DN25",1,"个"]
[1.6,"手动跑风阀","DN25",1,"个"]
[1.7,"螺纹法兰阀门","闸阀、灰铸铁、Z15T-16、DN25",1,"个"]
[1.8,"螺纹法兰阀门","泄水阀、铸铁、DN20",1,"个"]
[1.9,"散热器","铜铝复合柱翼500高",1,"片"]
[2,"超低噪声方形壁式轴流排风机","L=2000m3 /h",1,"台","配设防雨罩和防虫网"]
[2.1,"DN32采暖入口装置",null,1,"套"]

{"sheet":"汽车修理间","index":1,"n_rows":95,"n_cols":7,"rows_kept":95,"merged":[[0,0,0,5]]}
["S10尖山服务区材料统计"]
["编号","材料名称","规格型号","数量","单位","备注","单价/元"]
[1.1,"复合土工膜","质量≥600g/m2，膜材厚度≥0.3mm，CBR顶坡强度≥3.0KN，耐静水压≥0.6MPa",1,"㎡"]
[1.2,"混凝土","C20",1,"m3"]
[1.3,"混凝土","C40",1,"m3"]
[1.4,"加气混凝土块","300mm",1,"m3"]
[1.5,"加气混凝土块","200mm",1,"m3"]
[1.6,"炉渣",null,1,"m3"]
[1.7,"混凝土","C35",1,"m3"]
[1.8,"混凝土","C30",1,"m3"]
[1.9,"混凝土","C25",1,"m3"]
[2,"钢筋","HRB400，Φ6.5-10",1,"t"]
[2.1,"钢筋","HRB400，Φ12-14",1,"t"]
[2.2,"钢筋","HRB400，Φ16-25",1,"t"]
[2.3,"钢筋机械连接","直螺纹连接，钢筋直径:25mm以内",1,"个"]
[2.4,"钢筋机械连接","直螺纹连接，钢筋直径:20mm以内",1,"个"]
[2.6,"屋面卷材防水","4mm厚SBS防水层",1,"㎡"]
[2.7,"PVC管","DN100",1,"米"]
[2.9,"岩棉板","50厚岩棉板",1,"㎡"]
[3,"地板砖","参照图集",1,"㎡"]
[3.1,"地脚线砖","参照图集",1,"㎡"]
[3.2,"乳胶漆","内墙面漆",1,"㎡"]
[3.3,"铝合金方板吊顶","600*600",1,"㎡"]
[3.4,"氟碳漆",null,1,"㎡"]
[3.5,"防火卷帘(闸）门","钢质防火门卷帘门M-1  尺寸4500*4500",1,"樘","电动"]
[3.6,"防火卷帘(闸）门","钢质防火门卷帘门M-2    尺寸 3600*4500",1,"樘","电动"]
[3.7,"防火卷帘(闸）门","钢质防火门卷帘门M-3 尺寸 3200*3200",1,"樘","电动"]
[3.8,"钢质保温防盗防火门","1000*2400",1,"樘"]
[3.9,"金属（塑钢、断桥）窗","2100*1800",1,"樘"]
[4,"金属（塑钢、断桥）窗","1500*1500",1,"樘"]
[4.1,"金属（塑钢、断桥）窗","1200*1500",1,"樘"]
[1.1,"等电位箱",null,1,"台"]
[1.2,"配电箱","照明总配电箱",1,"台"]
[1.3,"配电箱","动力配电箱",1,"台"]
[1.4,"控制箱","与设备配套",1,"台"]
[1.5,"防尘防爆密封光照型灯","150W",1,"套"]
[1.6,"防尘防爆密封光照型灯","60W",1,"套"]
[1.7,"吸顶灯","60W",1,"套"]
[1.8,"吸顶灯","100W",1,"套","节能型"]
[1.9,"防尘防水灯","100W",1,"套","节能型"]
[2,"单管荧光灯","40W",1,"套","节能型"]
[2.1,"防水插座箱","XRZ301-4-06",1,"台"]
[2.2,"五孔插座","安全型双联二三级插座、P86Z14-25",1,"个"]
[2.3,"密闭双极开关","10A 250V",1,"个"]
[2.4,"密闭单极开关","10A 250V",1,"个"]
[2.5,"单极开关","10A 250V",1,"个"]
[2.6,"双联开关","10A 250V",1,"个"]
[2.7,"防爆双级开关","10A 250V",1,"个"]
[2.8,"防爆三级开关","10A 250V",1,"个"]
[2.9,"电动卷帘门接线盒",null,1,"个"]
[3,"电视插座","E31A75M",1,"个"]
[3.1,"电话插座","E31A75M",1,"个"]
[3.2,"电视前端箱（前端机柜）",null,1,"个"]
[3.3,"电力电线","BV-2.5",1,"米"]
[3.4,"电力电线","BV-4",1,"米"]
[3.5,"电力电线","RVB-2*0.5 ",1,"米"]
[3.6,"射频电缆","SYKV-75-5",1,"米"]
[3.7,"PVC管","DN20",1,"米"]
[3.8,"PVC管","DN25",1,"米"]
[3.9,"PVC管","DN15",1,"米"]
[4,"PVC管","DN50",1,"米"]
[4.1,"镀锌钢管","Φ50mm",1,"米"]
[4.2,"镀锌扁钢","-40mm",1,"米"]
[4.3,"镀锌圆钢","Φ12mm",1,"米"]
[1.1,"热镀锌钢管","DN20",1,"米","50mm厚岩棉管壳外加玻璃布乳化沥青保护层沥青漆二遍"]
[1.2,"热镀锌钢管","DN25",1,"米","50mm厚岩棉管壳外加玻璃布乳化沥青保护层沥青漆二遍"]
[1.3,"热镀锌钢管","DN32",1,"米","50mm厚岩棉管壳外加玻璃布乳化沥青保护层沥青漆二遍"]
[1.4,"热镀锌钢管","DN40",1,"米","50mm厚岩棉管壳外加玻璃布乳化沥青保护层沥青漆二遍"]
[1.5,"管道支架","L50角钢",1,"kg"]
[1.6,"两通锁闭温控调节阀","DN25",1,"个"]
[1.7,"手动跑风阀","DN25",1,"个"]
[1.8,"螺纹法兰阀门","闸阀、灰铸铁、Z15T-16、DN25",1,"个"]
[1.9,"螺纹法兰阀门","泄水阀、铸铁、DN20",1,"个"]
[2,"散热器","铜铝复合柱翼600高",1,"片"]
[2.1,"DN40采暖入口装置",null,1,"套"]
[1.1,"PP-R管","DN15",1,"米"]
[1.2,"PP-R管","DN20",1,"米"]
[1.3,"PP-R管","DN25",1,"米"]
[1.4,"PP-R管","DN32",1,"米"]
[1.5,"铸铁管","DN50",1,"米"]
[1.6,"铸铁管","DN75",1,"米"]
[1.7,"铸铁管","DN100",1,"米"]
[1.8,"螺纹阀门","Q11F-25T型DN15",1,"米","黄铜、球阀"]
[1.9,"螺纹阀门","Q11F-25T型DN20",1,"米","黄铜、球阀"]
[2,"螺纹法兰阀门","Z44T-10、DN32",1,"米","闸阀、灰铸铁"]
[2.1,"螺纹法兰阀门","H41T-16、DN32",1,"米","止回阀、灰铸铁"]
[2.2,"给、排水附(配)件","DN50",1,"米","带存水弯、不带存水弯:带存水弯，铝质"]
[2.3,"成品拖布池",null,1,"组"]
[2.4,"水龙头",null,1,"组"]
[2.5,"倒流防止器","DN15",1,"套"]
[2.6,"真空破坏器",null,1,"个"]
[2.7,"高压水枪",null,1,"套"]
[2.8,"管道支架","L50角钢",1,"kg"]
[2.9,"灭火器箱",null,1,"具"]
[3,"灭火器","MF/ABC4",1,"具"]

{"sheet":"综合楼","index":2,"n_rows":172,"n_cols":9,"rows_kept":172,"merged":[[0,0,0,7],[1,0,3,0],[1,1,3,2],[1,3,3,4],[1,5,3,5],[1,6,3,6],[1,7,3,7],[4,1,4,2],[4,3,4,4],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,16,2],[16,3,16,4],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,1,23,2],[23,3,23,4],[24,1,24,2],[24,3,24,4],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,1,27,2],[27,3,27,4],[28,1,28,2],[28,3,28,4],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[31,1,31,2],[31,3,31,4],[32,1,32,2],[32,3,32,4],[33,1,33,2],[33,3,33,4],[34,1,34,2],[34,3,34,4],[35,1,35,2],[35,3,35,4],[36,1,36,2],[36,3,36,4],[37,1,37,2],[37,3,37,4],[38,1,38,2],[38,3,38,4],[39,1,39,2],[39,3,39,4],[40,1,40,2],[40,3,40,4],[41,1,41,2],[41,3,41,4],[42,1,42,2],[42,3,42,4],[43,1,43,2],[43,3,43,4],[44,1,44,2],[44,3,44,4],[45,1,45,2],[45,3,45,4],[46,1,46,2],[46,3,46,4],[47,1,47,2],[47,3,47,4],[48,1,48,2],[48,3,48,4],[49,1,49,2],[49,3,49,4],[50,1,50,2],[50,3,50,4],[51,1,51,2],[51,3,51,4],[52,1,52,2],[52,3,52,4],[53,1,53,2],[53,3,53,4],[54,1,54,2],[54,3,54,4],[55,1,55,2],[55,3,55,4],[56,1,56,2],[56,3,56,4],[57,1,57,2],[57,3,57,4],[58,1,58,2],[58,3,58,4],[59,1,59,2],[59,3,59,4],[60,1,60,2],[60,3,60,4],[61,1,61,2],[61,3,61,4],[62,1,62,2],[62,3,62,4],[63,1,63,2],[63,3,63,4],[64,1,64,2],[64,3,64,4],[65,1,65,2],[65,3,65,4],[66,1,66,2],[66,3,66,4],[67,1,67,2],[67,3,67,4],[68,1,68,2],[68,3,68,4],[69,1,69,2],[69,3,69,4],[70,1,70,2],[70,3,70,4],[71,1,71,2],[71,3,71,4],[72,1,72,2],[72,3,72,4],[73,1,73,2],[73,3,73,4],[74,1,74,2],[74,3,74,4],[75,1,75,2],[75,3,75,4],[76,1,76,2],[76,3,76,4],[77,1,77,2],[77,3,77,4],[78,1,78,2],[78,3,78,4],[79,1,79,2],[79,3,79,4],[80,1,80,2],[80,3,80,4],[81,1,81,2],[81,3,81,4],[82,1,82,2],[82,3,82,4],[83,1,83,2],[83,3,83,4],[84,1,84,2],[84,3,84,4],[85,1,85,2],[85,3,85,4],[86,1,86,2],[86,3,86,4],[87,1,87,2],[87,3,87,4],[88,1,88,2],[88,3,88,4],[89,1,89,2],[89,3,89,4],[90,1,90,2],[90,3,90,4],[91,1,91,2],[91,3,91,4],[92,1,92,2],[92,3,92,4],[93,1,93,2],[93,3,93,4],[94,1,94,2],[94,3,94,4],[95,1,95,2],[95,3,95,4],[96,1,96,2],[96,3,96,4],[97,1,97,2],[97,3,97,4],[98,1,98,2],[98,3,98,4],[99,1,99,2],[99,3,99,4],[100,1,100,2],[100,3,100,4],[101,1,101,2],[101,3,101,4],[102,1,102,2],[102,3,102,4],[103,1,103,2],[103,3,103,4],[104,1,104,2],[104,3,104,4],[105,1,105,2],[105,3,105,4],[106,1,106,2],[106,3,106,4],[107,1,107,2],[107,3,107,4],[108,1,108,2],[108,3,108,4],[109,1,109,2],[109,3,109,4],[110,1,110,2],[110,3,110,4],[111,1,111,2],[111,3,111,4],[112,1,112,2],[112,3,112,4],[113,1,113,2],[113,3,113,4],[114,1,114,2],[114,3,114,4],[115,1,115,2],[115,3,115,4],[116,1,116,2],[116,3,116,4],[117,1,117,2],[117,3,117,4],[118,1,118,2],[118,3,118,4],[119,1,119,2],[119,3,119,4],[120,1,120,2],[120,3,120,4],[121,1,121,2],[121,3,121,4],[122,1,122,2],[122,3,122,4],[123,1,123,2],[123,3,123,4],[124,1,124,2],[124,3,124,4],[125,1,125,2],[125,3,125,4],[126,1,126,2],[126,3,126,4],[127,1,127,2],[127,3,127,4],[128,1,128,2],[128,3,128,4],[129,1,129,2],[129,3,129,4],[130,1,130,2],[130,3,130,4],[131,1,131,2],[131,3,131,4],[132,1,132,2],[132,3,132,4],[133,1,133,2],[133,3,133,4],[134,1,134,2],[134,3,134,4],[135,1,135,2],[135,3,135,4],[136,1,136,2],[136,3,136,4],[137,1,137,2],[137,3,137,4],[138,1,138,2],[138,3,138,4],[139,1,139,2],[139,3,139,4],[140,1,140,2],[140,3,140,4],[141,1,141,2],[141,3,141,4],[142,1,142,2],[142,3,142,4],[143,1,143,2],[143,3,143,4],[144,1,144,2],[144,3,144,4],[145,1,145,2],[145,3,145,4],[146,1,146,2],[146,3,146,4],[147,1,147,2],[147,3,147,4],[148,1,148,2],[148,3,148,4],[149,1,149,2],[149,3,149,4],[150,1,150,2],[150,3,150,4],[151,1,151,2],[151,3,151,4],[152,1,152,2],[152,3,152,4],[153,1,153,2],[153,3,153,4],[154,3,154,4],[155,3,155,4],[156,3,156,4],[157,3,157,4],[158,3,158,4],[159,3,159,4],[160,3,160,4],[161,3,161,4],[162,3,162,4],[163,3,163,4],[164,3,164,4],[165,3,165,4],[166,3,166,4],[167,3,167,4],[168,3,168,4],[169,3,169,4],[170,3,170,4],[171,3,171,4]]}
["材料明细"]
["序号","产品名称",null,"规格型号",null,"单位","数量","备注","单价/元"]
[]
[]
[1,"砂石",null,"1.5m厚砂夹石垫层 ",null,"m3",1]
[2,"复合土工膜",null,"质量≥600g/m2，膜材厚度≥0.3mm，CBR顶坡强度≥3.0KN，耐静水压≥0.6MPa",null,"m2",1,"两布一膜"]
[3,"商品混凝土",null,"C40\n",null,"m3",1]
[4,"商品混凝土",null,"C20\n",null,"m3",1]
[5,"商品混凝土",null,"C30\n",null,"m3",1]
[6,"商品混凝土",null,"C35\n",null,"m3",1]
[7,"商品混凝土",null,"C25\n",null,"m3",1]
[8,"加气混凝土块",null,"300\n",null,"m3",1]
[9,"加气混凝土块",null,200,null,"m3",1]
[10,"烧结多孔砖",null,"200\n",null,"m3",1]
[11,"卫生间防水导墙",{"$nulls":3},"m2",1]
[12,"垃圾道、通风道、烟道",null,"通风道",null,"m",1]
[13,"出屋面风帽",null,"出屋面风帽甘12J8-1",null,"座",1]
[14,"钢筋",null,"Φ10mm",null,"t",1]
[15,"钢筋",null,"HPB300，φ6-10",null,"t",1]
[16,"钢筋",null,"格:HRB400，6-10",null,"t",1]
[17,"钢筋",null,"HRB400，12-14",null,"t",1]
[18,"钢筋",null,"HRB400，16-25",null,"t",1]
[19,"钢筋",null,"HRB400，28-32",null,"t",1]
[20,"钢筋机械连接",null,"20mm以内",null,"个",1,"直螺纹连接"]
[21,"钢筋机械连接",null,"25mm以内",null,"个",1,"直螺纹连接"]
[22,"钢筋机械连接",null,"25mm以内",null,"个",1,"电渣压力焊接"]
[23,"钢筋机械连接",null,"32mm以内",null,"个",1,"电渣压力焊接"]
[24,"钢爬梯",null,"L50*50*5、Φ22",null,"t",1]
[25,"H钢",{"$nulls":3},"t",1]
[26,"屋面卷材防水",null,"3mm厚SBS防水层\n",null,"m2",1]
[27,"屋面卷材防水",null,"4mm厚SBS防水层\n",null,"m2",1]
[28,"挤塑聚苯板",null,"140mm",null,"m2",1]
[29,"PVC管",null,"110mm",null,"m",1]
[30,"钢化玻璃",null,"轻钢玻璃雨棚",null,"m2",1]
[31,"隔热楼地面",null,"200厚2：8白灰焦渣保温层",null,"m2",1]
[32,"岩棉板",null,"100mm",null,"m2",1]
[33,"地板砖",null,"见图集",null,"m2",1,"地砖地面（有防水），1.5厚聚氨酯防水涂膜"]
[34,"地板砖",null,"见图集",null,"m2",1]
[35,"石材地砖",null,"见图集",null,"m2",1]
[36,"防静电活动地板",null,"600*600",null,"m2",1]
[37,"地板砖",null,"见图集",null,"m2",1]
[38,"踢脚线",null,"见13J502-3-N03-①",null,"m2",1]
[39,"石材踢脚线",null,"见13J502-3-N02-④⑥",null,"m2",1]
[40,"花岗岩台阶面",null,"见05J909-SW8-台9A",null,"m2",1]
[41,"聚苯乙烯保温板",null,"容重20KG/m³，200mm",null,"m2",1]
[42,"真空镀铝聚酯薄膜",null,"0.2mm",null,"m2",1]
[43,"地板辐射采暖钢丝网",{"$nulls":3},"m2",1]
[44,"边界保温带",{"$nulls":3},"m",1]
[45,"釉面砖防水墙面",null,"规格见图集",null,"m2",1]
[46,"石材墙面",{"$nulls":3},"m2",1,"内墙9a门厅、商业、餐厅"]
[47,"石材柱面",null,"门厅柱",null,"m2",1,"门厅柱"]
[48,"腻子粉",{"$nulls":3},"m2",1]
[49,"乳胶漆",null,"白色乳胶漆\n",null,"m2",1,"公共走道、办公室、会议室、宿舍、司机之家等"]
[50,"热镀锌钢丝网",{"$nulls":3},"m2",1]
[51,"干挂石材墙面",null,"见05J909-WQ20-外墙25，干挂石材墙面",null,"m2",1]
[52,"玻璃幕墙",{"$nulls":3},"m2",1,"全玻竖明横，隐框玻璃幕墙，含五金"]
[53,"外墙 真石漆",null,"见05J909-WQ10-外墙13F  真石漆",null,"m2",1]
[54,"卫生间、淋浴间隔断",null,"成品隔断",null,"m2",1]
[55,"乳胶漆",null,"1.白色乳胶漆",null,"m2",1]
[56,"防火纸面石膏板吊顶",null,"600*600",null,"m2",1]
[57,"铝合金方板吊顶",null,"300*300",null,"m2",1]
[58,"矿棉装饰吸声板吊顶",null,"600*600",null,"m2",1]
[59,"铝方通",{"$nulls":3},"m2",1,"金属幕墙背面"]
[60,"钢质丙级防火门",null,"700*2100",null,"樘",1]
[61,"钢质乙级防火门",null,"1000*2200",null,"樘",1]
[62,"安全玻璃门",null,"800*2100",null,"樘",1]
[63,"木质门",null,"1000*2200",null,"樘",1]
[64,"木质门",null,"1500*2200",null,"樘",1]
[65,"安全玻璃门",null,"1500*2700",null,"樘",1]
[66,"木质门",null,"1500*4800",null,"樘",1]
[67,"钢质甲级防火门",null,"1500*2200",null,"樘",1]
[68,"金属（塑钢、断桥）窗",null,"1500*1800",null,"樘",1,"断桥铝合金中空玻璃窗，纱窗"]
[69,"金属（塑钢、断桥）窗",null,"1500*4800",null,"樘",1,"断桥铝合金中空玻璃窗，纱窗"]
[70,"钢质防火窗",null,"2100*2100",null,"樘",1,"带纱窗"]
[71,"金属（塑钢、断桥）窗",null,"1500*900",null,"樘",1,"断桥铝合金中空玻璃窗，纱窗"]
[72,"钢质防火窗",null,"1500*1800",null,"樘",1,"带纱窗"]
[73,"钢质防火窗",null,"1500*4800",null,"樘",1,"带纱窗"]
[74,"铝合金防寒门斗",null,"铝合金防寒门斗",null,"樘",1]
[75,"不锈钢扶手",null,"12J6-17-1",null,"m",1]
[76,"不锈钢栏杆",null,"12J5-2-27",null,"m",1]
[77,"不锈钢扶手",null,"06J403-1-B27-36",null,"m",1]
[78,"洗漱大理石台面",null,"12J10-123-1",null,"m2",1]
[79,"镜面玻璃",null,"镜面玻璃",null,"m2",1]
[80,"花岗岩板",{"$nulls":3},"m2",1,"石材窗台板"]
[81,"成品窗帘盒",{"$nulls":3},"m",1]
[82,"不锈钢扶手、栏杆、栏板",null,"12J6-79、12J6-85",null,"m",1]
[83,"不锈钢护窗栏杆",null,"高度1100mm",null,"m2",1]
[84,"挂钩",null,"卫生间挂钩",null,"个",1]
[85,"LOGO",null,"5.33m*4.264m，支架钢材品种、规格:100*50*3热镀锌钢通、50*50*3热镀锌钢通、钢板",null,"个",1,"冲孔铝合金板镶嵌外露灯珠，支架钢材品种、规格:100*50*3热镀锌钢通、50*50*3热镀锌钢通、钢板"]
[86,"标志字 ",null,"3m*3m，支架钢材品种、规格:100*50*3热镀锌钢通、50*50*3热镀锌钢通、钢板",null,"个",1,"冲孔铝合金板镶嵌外露灯珠，支架钢材品种、规格:100*50*3热镀锌钢通、50*50*4热镀锌钢通、钢板"]
[87,"英文字体",null,"0.8m*0.6m",null,"个",1,"冲孔铝合金板镶嵌外露灯珠，支架钢材品种、规格:100*50*3热镀锌钢通、50*50*5热镀锌钢通、钢板"]
[88,"标志字",null,"1.36m*1.5m",null,"个",1,"冲孔铝合金板镶嵌外露灯珠，支架钢材品种、规格:100*50*3热镀锌钢通、50*50*6热镀锌钢通、钢板"]
[89,"英文字体",null,"0.65m*0.4m",null,"个",1,"冲孔铝合金板镶嵌外露灯珠，支架钢材品种、规格:100*50*3热镀锌钢通、50*50*7热镀锌钢通、钢板"]
[90,"不锈钢操作台",null,"800mm",null,"m2",1]
[91,"成品商用组合灶",null,"成品商用组合灶",null,"套",1]
[92,"厨柜",null,"厨柜",null,"m2",1]
[93,"消毒柜",null,"消毒柜",null,"套",1]
[94,"冰柜",null,"冰柜",null,"套",1]
[95,"洗碗机、灶具等配套",null,"洗碗机、灶具等配套",null,"项",1]
[96,"手机加油站",null,"500*55*1800",null,"套",1]
[97,"信息查询触摸屏",null,"42\"",null,"套",1]
[98,"19\"机柜",{"$nulls":3},"套",1]
[99,"镀锌钢管",null,"DN50",null,"米",1]
[100,"室内LED信息大屏",null,"6000*4000",null,"套",1]
[101,"LED信息大屏控制计算机",{"$nulls":3},"套",1]
[102,"室内高清网络半球摄像机",null,"1384*1076/12vDC/24vDC/7W",null,"套",1]
[103,"电源线",null,"BV3*4",null,"米",1]
[104,"电力电缆",null,"YJV5*16",null,"米",1]
[105,"电力电缆",null,"YJV22-5*16",null,"米",1]
[106,"电力电缆",null,"YJV22-4*35—+1*16",null,"米",1]
[107,"网线",null,"UTP5 4*（2*0.5）",null,"米",1]
[108,"局部等电位箱",null,"TD28",null,"台",1]
[109,"总等电位箱",null,"TD28",null,"台",1]
[110,"照明配电箱",null,"PZ30、XRM301",null,"台",1]
[111,"动力照明配电箱",null,"PZ30、XRM301",null,"台",1]
[112,"电源自动切换箱",{"$nulls":3},"台",1]
[113,"浴霸",null,"1.5KW，一体式",null,"台",1]
[114,"防水除尘灯",null,"LED,12W",null,"盏",1]
[115,"LED面板灯",null,"LED,40W",null,"盏",1]
[116,"天棚灯",null,"LED,12W",null,"盏",1]
[117,"筒灯",null,"LED,5W",null,"盏",1]
[118,"筒灯",null,"LED,12W",null,"盏",1]
[119,"安全型带接地插孔密闭三相插座",null,"25A,380V",null,"个",1]
[120,"安全型带保护接地点防水洗脸盆单项插座",null,"10A，250",null,"个",1]
[121,"安全型双联二三级暗装插座",null,"NEW7-111",null,"个",1]
[122,"安全型带安全门防水插座箱",null,"XRZ301-3-01",null,"个",1]
[123,"安全型双联二三级防水密闭插座",null,"NEW8-448A",null,"个",1]
[124,"安全型柜式空调插座",null,"16A,250V",null,"个",1]
[125,"安全型壁挂式空调插座",null,"16A,250V",null,"个",1]
[126,"延迟开关",{"$nulls":3},"个",1]
[127,"密闭三级开关",null,"10A，250v",null,"个",1]
[128,"密闭双级开关",null,"10A，250v",null,"个",1]
[129,"密闭单三级开关",null,"10A，250v",null,"个",1]
[130,"开关",null,"10A，250v",null,"个",1]
[131,"双联开关",null,"10A，250v",null,"个",1]
[132,"三联开关",null,"10A，250v",null,"个",1]
[133,"四联开关",null,"10A，250v",null,"个",1]
[134,"BV导线",null,"BV 2.5",null,"米",1]
[135,"BV导线",null,"BV4.0",null,"米",1]
[136,"护套屏蔽软线",null,"NH-RVVP1.5",null,"米",1]
[137,"电力电缆",null,"YJV22-4*35+1*16",null,"米",1]
[138,"电力电缆",null,"YJV22-4*95+1*50",null,"米",1]
[139,"电力电缆",null,"YJV22-4*50+1*25",null,"米",1]
[140,"电力电缆",null,"YJV22-4*240+1*120",null,"米",1]
[141,"电力电缆",null,"YJV22-5*16",null,"米",1]
[142,"电力电缆",null,"YJV-5*17",null,"米",1]
[143,"电力电缆",null,"YJV4*35+1*16",null,"米",1]
[144,"电力电缆",null,"YJV4*25+1*16",null,"米",1]
[145,"电力电缆",null,"YJV5*10",null,"米",1]
[146,"电力电缆",null,"YJV5*6",null,"米",1]
[147,"电力电缆",null,"NH-YJV4*35+1*16",null,"米",1]
[148,"电力电缆",null,"NH-BV2.5",null,"米",1]
[149,"电力电缆",null,"BV6",null,"米",1]
[150,"护套线",null,"RBV2*0.5",null,"米",1]
[151,null,"铜芯聚录乙烯绝缘平行软线","UTP5e （2*0.5）",null,"米",1]
[152,null,"射频同轴电缆","SYKV-75-9",null,"米",1]
[153,null,"射频同轴电缆","SYKV-75-5",null,"米",1]
[154,null,"通信电缆","HYV20,50*(2*0.5)",null,"米",1]
[155,null,"PVC管","20mm",null,"米",1]
[156,null,"镀锌钢管","SC100",null,"米",1]
[157,null,"镀锌钢管","SC150",null,"米",1]
[158,null,"镀锌钢管","SC50",null,"米",1]
[159,null,"镀锌钢管","SC40",null,"米",1]
[160,null,"镀锌钢管","SC20",null,"米",1]
[161,null,"镀锌钢管","SC80",null,"米",1]
[162,null,"PVC管","25mm",null,"米",1]
[163,null,"镀锌钢管","SC32",null,"米",1]
[164,null,"桥架","200*100",null,"米",1]
[165,null,"总配线架",null,null,"台",1]
[166,null,"信息插座","E31A75M",null,"个",1]
[167,null,"电视插座","E31A75M",null,"个",1]
[168,null,"电话插座","E31A75M",null,"个",1]

{"sheet":"生活蓄水池","index":3,"n_rows":19,"n_cols":6,"rows_kept":19,"merged":[[0,0,0,5]]}
["材料明细表"]
["工程名称：生活蓄水池"]
["序号","产品名称","规格及型号","单位","数量","单价"]
[1,"控制箱","见图纸","台",1]
[2,"水池液位计传送器",null,"支",1]
[3,"铜芯电力电缆","YJV22-1KV-5*4\n","m",1]
[4,"焊接钢管","DN25\n","m",1]
[5,"电气配线","NH-RVVP-4*1.5\n","m",1]
[6,"焊接钢管","DN20","m",1]
[7,"内外涂塑钢管","DN100\n","m",1]
[8,"闸阀","Z44T-10、DN100","个",1]
[9,"止回阀","H44X-16、DN100","个",1]
[10,"生活潜水泵","H=32.0m N=4KW Q=25m3/h","台",1]
[11,"混凝土","C35","m3",1]
[12,"混凝土","C15","m3",1]
[13,"SBS防水","厚4mm","m2",1]
[14,"钢筋","三级钢筋","t",1]
[15,"实心砖","240mm墙","m3",1]
[16,"混凝土","C25","m3",1]

{"sheet":"设备用房","index":4,"n_rows":247,"n_cols":6,"rows_kept":247,"merged":[[0,0,0,5]]}
["材料明细表"]
["序号","产品名称","规格及型号","单位","数量","单价"]
[1,"热镀锌钢管","\nDN25\n","m",1]
[2,"热镀锌钢管","DN25\n","m",1]
[3,"热镀锌钢管","\nDN32\n","m",1]
[4,"型钢支架",null,"kg",1]
[5,"自动排气阀","DN25\n","个",1]
[6,"两通锁闭温控调节阀","DN25","个",1]
[7,"手动跑风阀","DN25","个",1]
[8,"闸阀","Z15T-16、DN25","个",1]
[9,"泄水阀","DN20","个",1]
[10,"其他成品散热器","铜铝复合柱翼500高散热器","片",1]
[11,"采暖导入口","DN25","组",1]
[12,"壁式轴流通风机阻燃防爆型","XBDZ-2.5#,功率0.09KW，额定新风量800m3 /h，P=68Pa","台",1]
[13,"壁式轴流通风机阻燃防爆型","XBDZ-2.5#,功率0.09KW，额定新风量800m3 /h，P=42Pa","台",1]
[14,"壁式轴流通风机阻燃防爆型","XBDZ-2.5#,功率0.025KW，额定新风量600m3 /h，P=42Pa","台",1]
[15,"建筑与装饰工程",null,null,1]
[16,"复合土工膜","单位面积质量≥600g/m2，膜材厚度≥0.3mm，CBR顶坡强度≥3.0KN，耐静水压≥0.6MPa","m2",1]
[17,"混凝土","C20","m3",1]
[18,"混凝土","C40","m3",1]
[19,"混凝土加气块",300,"m3",1]
[20,"混凝土加气块",200,"m3",1]
[21,"炉渣","200厚","m3",1]
[22,"混凝土","C35","m3",1]
[23,"混凝土","C30","m3",1]
[24,"混凝土","C25","m3",1]
[25,"钢筋","HRB400，6.5-10","t",1]
[26,"钢筋","HRB400，12-14","t",1]
[27,"钢筋","HRB400，16-25","t",1]
[28,"钢筋机械连接",null,"个",1]
[29,"钢筋机械连接",null,"个",1]
[30,"钢爬梯","钢爬梯制作、安装","t",1]
[31,"SBS防水材料","3+4mm厚","m2",1]
[32,"挤塑聚苯板","80mm","m2",1]
[33,"PVC管","铸铁雨水口、塑料落水管DN100","m",1]
[34,"隔热楼地面","200厚2：8白灰焦渣保温层","m2",1]
[35,"岩棉保温一体板","50厚岩棉保温一体板","m2",1]
[36,"超细玻璃棉","50厚超细玻璃棉","m2",1]
[37,"地板砖","600*600","m2",1]
[38,"踢脚线","见12J1-1-7-1","m2",1]
[39,"乳胶漆","见05J909-NQ12-内墙7A1","m2",1]
[40,"挤塑聚苯板檐线","规格100mm*100mm","m",1]
[41,"乳胶漆","05J909-DP7-棚7A（白色乳胶漆）","m2",1]
[42,"矿棉板吊顶","600x600","m2",1]
[43,"钢质甲级防火门","1000*2100","樘",1]
[44,"钢质甲级防火门","1500*2100","樘",1]
[45,"钢质甲级防火门","1800*2700","樘",1]
[46,"钢制甲级防火窗","1500*1800","樘",1]
[47,"钢制甲级防火窗","1500*900","樘",1]
[48,"窗台板","甘12J1-4","m2",1]
[49,"空气源热泵系统",null,null,1]
[50,"超低温空气源热泵机组（室外机）","DNL-Y1400/NSN1-H\n额定制热量:140kw额定制热功率:46.67kw","台",1]
[51,"供暖热计量装置","Q=16m3/h","块",1]
[52,"一次供热循环泵（变频）","FLG-125（I） Q=57.5m3/h N=7.5kw H=24m","台",1]
[53,"一次供热循环泵（变频）","FLG-80-200A Q=27.5m3/h N=3.5kw H=32m","台",1]
[54,"缓冲水箱","3m3 工作压力1.0MPa","台",1]
[55,"全自动钠离子软水器","（t/h):Q=2t/h，进水压力0.25MPa","台",1]
[56,"软化水箱","2m3 ","台",1]
[57,"二次供热补水泵","FLG-20-160 Q=2.5m3/h N=0.75kw H=32m","台",1]
[58,"立式（囊式）膨胀定压罐","RSN800 V=0.82m3,工作压力1.0MPa","套",1]
[59,"超声波热量表（供热）","Q=55m3/h","块",1]
[60,"超声波","Q=2m3/h","块",1]
[61,"电动三通阀","工作压力1.0MPa DN125","个",1]
[62,"直通除污器","工作压力1.0MPa DN125","组",1]
[63,"电接点压力表","磁助型0-0.6至60级","台",1]
[64,"旋翼式水表","DN40","个",1]
[65,"无缝钢管","DN125 0.6MPa","m",1]
[66,"无缝钢管","DN100 0.6MPa","m",1]
[67,"无缝钢管","DN70 0.6MPa","m",1]
[68,"焊接钢管","DN50 0.6MPa","m",1]
[69,"焊接钢管","DN40 0.6MPa","m",1]
[70,"焊接钢管","DN32 0.6MPa","m",1]
[71,"焊接钢管","DN20 0.6MPa","m",1]
[72,"超细玻璃棉","50mm","m3",1]
[73,"超细玻璃棉","50mm","m3",1]
[74,"超细玻璃棉","50mm","m3",1]
[75,"镀锌铁皮","50mm","m2",1]
[76,"管道支架",null,"kg",1]
[77,"Y型过滤器","DN70","个",1]
[78,"橡胶可挠性接头","DN70","个",1]
[79,"截止阀","J41T-16、DN70","个",1]
[80,"截止阀","J41T-16、DN40","个",1]
[81,"橡胶可挠性接头","DN40","个",1]
[82,"闸阀","Z41T-16、DN20","个",1]
[83,"闸阀","Z41T-16、DN32","个",1]
[84,"泄水电磁阀","DN20","个",1]
[85,"安全阀","A47H-10、DN20","个",1]
[86,"Y型过滤器","DN40","个",1]
[87,"止回阀","H44T-16、DN40","个",1]
[88,"蝶阀","D341H-16、DN150","个",1]
[89,"止回阀","H44T-16型、DN150","个",1]
[90,"橡胶可挠性接头","DN150","个",1]
[91,"蝶阀","D341H-16、DN125","个",1]
[92,"止回阀","H44T-16型、DN125","个",1]
[93,"橡胶可挠性接头","DN125","个",1]
[94,"闸阀","Z44T-10、DN25","个",1]
[95,"压力表",null,"个",1]
[96,"自动排气阀","DN25","个",1]
[97,"温度计","WNG-12-200°C型","支",1]
[98,"给排水、消防工程",null,null,1]
[99,"无缝铝合金衬塑pp-r管","DN150","m",1]
[100,"无缝铝合金衬塑pp-r管","DN100","m",1]
[101,"无缝铝合金衬塑pp-r管","DN50","m",1]
[102,"无缝铝合金衬塑pp-r管","DN32","m",1]
[103,"钢管","DN50","m",1]
[104,"钢管","DN100","m",1]
[105,"不锈钢水箱","3000*2000*3000mm","台",1]
[106,"水箱自洁消毒器","WTS-2A","台",1]
[107,"给水变频控制柜","600*500*1600","台",1]
[108,"给水变频设备供水泵"," Q=7.5-15M3/h，H=0.27-0.42MPa，N=7.5KW","台",1]
[109,"仪表阀门"," DN50","个",1]
[110,"闸阀","Z44T-10、DN150","个",1]
[111,"止回阀","H41T-16、DN150","个",1]
[112,"闸阀","Z44T-10、DN100","个",1]
[113,"止回阀","H41T-16、DN100","个",1]
[114,"闸阀","Z44T-10、DN50","个",1]
[115,"止回阀","H41T-16、DN50","个",1]
[116,"球阀","Q11F-25T型DN50","个",1]
[117,"球阀","Q11F-25T型DN32","个",1]
[118,"倒流防止器","DN32","套",1]
[119,"过滤器","DN50","个",1]
[120,"水表","DN50","个",1]
[121,"管道支架",null,"kg",1]
[122,"落地式泄水池","500*500*250","组",1]
[123,"地漏","DN75","组",1]
[124,"地面扫除口"," DN100","组",1]
[125,"铸铁管","DN100","m",1]
[126,"管道支架",null,"kg",1]
[127,"七氟丙烷半固定柜 ","HFC-227eaGQQ40/2.5C","套",1]
[128,"七氟丙烷半固定柜","HFC-227eaGQQ60/2.5C","套",1]
[129,"七氟丙烷半固定柜","HFC-227eaGQQ90/2.5C","套",1]
[130,"七氟丙烷半固定柜 "," HFC-227eaGQQ120/2.5C","套",1]
[131,"灭火器箱",null,"具",1]
[132,"灭火器","MF/ABC3","具",1]
[133,"电气工程",null,null,1]
[134,"照明配电箱","见图纸","台",1]
[135,"控制箱","见图纸","台",1]
[136,"变频控制柜","见图纸","台",1]
[137,"可燃气体报警控制器","见图纸","台",1]
[138,"电锅炉控制柜","见图纸","台",1]
[139,"动力配电箱","见图纸","台",1]
[140,"总等电位箱","见图纸","台",1]
[141,"总等电位箱","见图纸","台",1]
[142,"LED 天棚灯","1*30W","套",1]
[143,"LED壁灯","1*18W","套",1]
[144,"LED防水防尘灯","1*24W","套",1]
[145,"LED双管荧光灯","2*24W  ","套",1]
[146,"LED防爆灯","1*40W","套",1]
[147,"安全型双联二三级插座","五孔插座 /P86Z14-25","个",1]
[148,"单极开关","10A 250V","个",1]
[149,"三极开关","10A 250V","个",1]
[150,"双联开关","10A 250V","个",1]
[151,"密闭三极开关","10A 250V","个",1]
[152,"防爆三级开关","10A 250V","个",1]
[153,"电视插座","E31A75M","个",1]
[154,"信息插座","E31A75M","个",1]
[155,"楼层配线箱","见图纸","个",1]
[156,"电话插座","E31A75M","个",1]
[157,"壁龛交接箱","见图纸","台",1]
[158,"电视前端箱","见图纸","个",1]
[159,"双电源切换箱","见图纸","台",1]
[160,"电气配线","NH-BV-2.5","m",1]
[161,"铜芯电力电缆","NH-YJV-1KV-5*6","m",1]
[162,"铜芯电力电缆","YJV-1KV-5*16","m",1]
[163,"电气配线","RVB-2*0.5   ","m",1]
[164,"电气配线","BV-2.5    ","m",1]
[165,"射频电缆","SYKV-75-5","m",1]
[166,"双绞线缆","HYV20-10(2*0.5)","m",1]
[167,"五类4对对绞线","UTP5e-4*（2*0.5）","m",1]
[168,"射频电缆","SYKV-75-9","m",1]
[169,"铜芯电力电缆","YJV-1KV-4*50+1*25","m",1]
[170,"铜芯电力电缆","YJV22-1KV-5*16","m",1]
[171,"电气配线","NH-RVVP1.5","m",1]
[172,"电气配线","BV-4","m",1]
[173,"铜芯电力电缆","YJV-1KV-5*10","m",1]
[174,"铜芯电力电缆","YJV-1KV-5*6","m",1]
[175,"铜芯电力电缆","YJV-1KV-4*25+1*16","m",1]
[176,"铜芯电力电缆","JHS-3*4","m",1]
[177,"铜芯电力电缆","YJV-1KV-5*4","m",1]
[178,"电气配线","RVVP1.5","m",1]
[179,"电气配线","NH-BV4","m",1]
[180,"铜芯电力电缆","NH-YJV-1KV-5*10","m",1]
[181,"电气配线","RVS-2*0.5   ","m",1]
[182,"电气配线","NH-BV-10","m",1]
[183,"铜芯电力电缆","YJV-4*150+1*70","m",1]
[184,"穿线管","PVC20","m",1]
[185,"穿线管","PVC25","m",1]
[186,"焊接钢管","DN40","m",1]
[187,"焊接钢管","DN50","m",1]
[188,"焊接钢管","DN15","m",1]
[189,"焊接钢管","DN20","m",1]
[190,"焊接钢管","DN25","m",1]
[191,"焊接钢管","DN32","m",1]
[192,"焊接钢管","DN125","m",1]
[193,"避雷网及接地装置","Φ12镀锌圆钢、镀锌扁钢 40*4、镀锌钢管 Φ50","套",1]
[194,"应急照明集中电源（A型）","1KW，初装时间>180   ","台",1]
[195,"消防应急标志灯（A型）","1W  LED","套",1]
[196,"消防应急标志灯（A型）","3W  LED","套",1]
[197,"可燃气体检测器",null,"套",1]
[198,"钢制线槽","100*60","m",1]
[199,"点型探测器","感烟","个",1]
[200,"点型探测器","感温","个",1]
[201,"指示灯",null,"套",1]
[202,"火灾警铃",null,"个",1]
[203,"启止器",null,"台",1]
[204,"紧急启停按钮",null,"个",1]
[205,"声光报警器",null,"个",1]
[206,"电磁阀",null,"个",1]
[207,"气体灭火控制器","见图纸","个",1]
[208,"直流电源","见图纸","台",1]
[209,"多股双绞铜芯阻燃屏蔽电线","PRA-DJYAP-2*1.0+1*1.5","m",1]
[210,"电气配线","ZR-BV4     ","m",1]
[211,"铜芯电力电缆","NH-YJV22-1KV-5*6","m",1]
[212,"电气配线","ZR-BV6     ","m",1]
[213,"五类4对对绞线","UTP5e-4*（2*0.5）","m",1]
[214,"消防双电源切换箱 ","见图纸","台",1]
[215,"干式变压器(带防护外壳)","SCB12-250/10","台",1]
[216,"干式变压器(带防护外壳)","SCB12-630/10","台",1]
[217,"跌落式熔断器","RW3、7、9-10","个",1]
[218,"避雷器","HY5WZ-12.7/45","组",1]
[219,"隔离开关","GN19-10/400-630","组",1]
[220,"盘型悬式绝缘子","XP-70","处",1]
[221,"支柱绝缘子","ZPB-10","处",1]
[222,"角钢支架",null,"根",1]
[223,"铜母线","TMY-50*5","m",1]
[224,"铜母线","TMY-80*6.3","m",1]
[225,"铜母线","TMY-100*8","m",1]
[226,"铜母线","TMY-80*8","m",1]
[227,"高压成套配电柜","HXGN15-12F-02","台",1]
[228,"低压开关柜(屏）","XLGS(GCS)-23(改)","台",1]
[229,"低压电容器柜","GCS-34B","台",1]
[230,"支柱绝缘子","ZPB-10","处",1]
[231,"角钢支架","角钢","根",1]
[232,"自启动柴油发电机组","400KW-Z自起动柴油发电机组","台",1]
[233,"柴油储备装置","柴油储备装置","台",1]
[234,"排风机","FBD40-A2-400","台",1]
[235,"铜芯电力电缆","YJV-10KV-3*35","m",1]
[236,"铜芯电力电缆","YJV-10KV-3*50","m",1]
[237,"铜芯电力电缆","YJV-10KV-3*95","m",1]
[238,"铜芯电力电缆","NH-YJV-4*240+1*120","m",1]
[239,"铜芯电力电缆","NH-YJV-4*300+1*150","m",1]
[240,"电气配线","BV-1.5     ","m",1]
[241,"焊接钢管","DN150","m",1]
[242,"焊接钢管","DN100","m",1]
[243,"焊接钢管","DN50","m",1]
[244,"高压绝缘垫板","高压绝缘垫板","m2",1]
[245,"封闭母线","630A","m",1]

{"sheet":"污水处理间","index":5,"n_rows":63,"n_cols":6,"rows_kept":63,"merged":[[0,0,0,5]]}
["污水处理间材料明细"]
["序号","产品名称","规格及型号","单位","数量","单价"]
[1,"混凝土","C25","m3",1]
[3,"复合土工膜","单位面积质量≥600g/m2，膜材厚度≥0.3mm，CBR顶坡强度≥3.0KN，耐静水压≥0.6MPa","m2",1]
[4,"混凝土加气块",300,"m3",1]
[5,"混凝土加气块",200,"m3",1]
[6,"混凝土","C20","m3",1]
[7,"混凝土","C40","m3",1]
[8,"炉渣",null,"m3",1]
[9,"混凝土","C30","m3",1]
[10,"钢筋","HRB400，6-10","t",1]
[11,"钢筋","HRB400，12-14","t",1]
[12,"钢筋","HRB400，16-25","t",1]
[13,"钢筋机械连接","钢筋直径:25mm以内","个",1]
[14,"钢筋机械连接","钢筋直径:25mm以内","个",1]
[15,"钢爬梯","钢爬梯制作","t",1]
[16,"SBS防水材料","3+4mm厚SBS防水层","m2",1]
[17,"挤塑聚苯板","80mm","m2",1]
[18,"PVC管","铸铁雨水口、DN100","m",1]
[19,"隔热楼地面","200厚2：8白灰焦渣保温层","m2",1]
[20,"岩棉保温一体板","80厚岩棉保温一体板","m2",1]
[21,"乳胶漆","内墙","m2",1]
[22,"乳胶漆","白色乳胶漆","m2",1]
[23,"电动防火卷闸门","1000*2100","樘",1]
[24,"钢质保温防盗门","1500*2400","樘",1]
[25,"钢质乙级防火门","1800*2400","樘",1]
[26,"断桥铝合金中空玻璃窗","2100*1800","樘",1]
[27,"窗台板","甘12J1-4","m2",1]
[28,"给排水、设备工程（100T）",null,null,1]
[29,"MPF(自养+异养反硝化)一体化污水处理设备","100T/D","套",1]
[30,"灭火器箱",null,"具",1]
[31,"灭火器","MF/ABC4","具",1]
[32,"电气工程",null,null,1]
[33,"总等电位箱","见图纸","台",1]
[34,"污水处理设备控制配电柜","与厂家设备成套提供","台",1]
[35,"污水处理设备控制柜","与厂家设备成套提供","台",1]
[36,"单相防水密闭插座","五孔插座 /16A 250V","个",1]
[37,"LED 天棚灯","1*30W","套",1]
[38,"广照型防水防尘灯","1*12W","套",1]
[39,"密闭双极开关","10A 250V","个",1]
[40,"电气配线","BV-2.5    ","m",1]
[41,"电气配线","BV-4","m",1]
[42,"电气配管","PVC20","m",1]
[43,"铜芯电力电缆","YJV22-1KV-4*25+1*16","m",1]
[44,"铜芯电力电缆","YJV-1KV-5*10","m",1]
[45,"铜芯电力电缆","YJV-1KV-4*4","m",1]
[46,"焊接钢管","DN50","m",1]
[47,"焊接钢管","DN40","m",1]
[48,"焊接钢管","DN32","m",1]
[49,"避雷网及接地装置","Φ12镀锌圆钢、镀锌扁钢 40*4\n、镀锌钢管 Φ50","套",1]
[50,"采暖、通风工程",null,null,1]
[51,"内外热镀锌钢管(不保温)","DN20","m",1]
[52,"内外热镀锌钢管(不保温)","DN25","m",1]
[53,"内外热镀锌钢管(不保温)","DN32","m",1]
[54,"内外热镀锌钢管(保温)","DN32","m",1]
[55,"管道支架","型钢支架","kg",1]
[56,"手动调节阀","DN25","个",1]
[57,"手动跑风阀","DN25","个",1]
[58,"闸阀","Z15T-16、DN25","个",1]
[59,"泄水阀","DN20","个",1]
[60,"其他成品散热器","铜铝复合柱翼500高散热器","片",1]
[61,"采暖导入口","DN32","组",1]
[62,"超低噪声方形壁式轴流排风机","L=1800m3 /h","台",1]

{"sheet":"蓄水池","index":6,"n_rows":132,"n_cols":7,"rows_kept":132,"merged":[[0,0,0,5]]}
["材料明细表"]
["工程名称：服务区蓄水池--建筑与装饰工程"]
["序号","产品名称","规格及型号","单位","数量","单价"]
[1,"混凝土","C35","座",1]
[2,"钢筋","三级钢筋","t",1]
[3,"混凝土","C20 ","m2",1]
[4,"实心砖",240,"m3",1]
[5,"实心砖",240,"m3",1]
[6,"混凝土","C25","m3",1]
[7,"钢支架",null,"t",1]
[8,"不锈钢盖板",null,"t",1]
[9,"零星钢构件",null,"t",1]
[10,"混凝土","C10","m2",1]
[11,"零星钢构件","止水螺杆","t",1]
[12,"钢质甲级防火门",null,"m2",1]
[13,"混凝土","C30","m2",1]
[14,"消防池地砖",null,"m2",1,null,"消防水池"]
[15,"水泥砂浆踢脚线","踢脚线高度:150mm ","m",1]
[16,"玻璃钢雨棚","8+1.52PVB+8厚夹胶玻璃","m2",1]
[17,"乳胶漆",null,"m2",1]
[18,"金属栏杆（楼梯)","不锈钢：甘12J6-27-1","m",1]
[19,"给排水、消防工程",null,null,1]
[20,"内涂PE钢塑复合管","DN100","m",1]
[21,"内外热浸镀锌钢管","DN150","m",1]
[22,"内外热浸镀锌钢管","DN200","m",1]
[23,"内外热浸镀锌钢管","DN100","m",1]
[24,"内外热浸镀锌钢管","DN250","m",1]
[25,"内外热浸镀锌钢管","DN32","m",1]
[26,"内外热浸镀锌钢管","DN150","m",1]
[27,"内外热浸镀锌钢管","DN150","m",1]
[28,"泄压阀","Y45X-16T DN100","组",1]
[29,"法兰液压式水位控制阀","SKF100-3、DN100","个",1]
[30,"截止阀","J11T-16 DN25","个",1]
[31,"截止阀","J11T-16 DN32","个",1]
[32,"橡胶软接头","DN100","个",1]
[33,"橡胶软接头","DN200","个",1]
[34,"橡胶软接头","DN250","个",1]
[35,"橡胶软接头","DN150","个",1]
[36,"橡胶软接头","DN32","个",1]
[37,"橡胶软接头","DN50","个",1]
[38,"止回阀","H44X-16、DN150","个",1]
[39,"闸阀","Z41H-16C、DN100","个",1]
[40,"蝶阀","A型DN150","个",1]
[41,"止回阀","H44X-16、DN100","个",1]
[42,"蝶阀","DN100","个",1]
[43,"闸阀","Z41H-16C、DN150","个",1]
[44,"闸阀","Z41H-16C、DN200","个",1]
[45,"蝶阀","A型DN200","个",1]
[46,"闸阀","Z41H-16C、DN250","个",1]
[47,"止回阀","H44X-16、DN200","个",1]
[48,"闸阀","Z41H-16C、DN70","个",1]
[49,"闸阀","Z41H-16C、DN50","个",1]
[50,"止回阀","H44X-16、DN50","个",1]
[51,"旋流防止器","DN50","套",1]
[52,"旋流防止器"," DN100","套",1]
[53,"旋流防止器","DN250","套",1]
[54,"压力表",null,"台",1]
[55,"防虫网罩","DN150","个",1]
[56,"柔性套管","DN150","个",1]
[57,"柔性套管","DN200","个",1]
[58,"柔性套管","DN100","个",1]
[59,"柔性套管","DN50","个",1]
[60,"柔性套管","DN25","个",1]
[61,"钢制弯头","DN100","组",1]
[62,"钢制弯头","DN150","组",1]
[63,"室内消火栓给水泵","XBD7.5/25-100L-KQ H=75m N=37KW Q=25L/s","台",1]
[64,"喷淋泵","XBD10/60-150L-KQ  H=100m N=90KW Q=60L/s","台",1]
[65,"室外消火栓给水泵","XBD4.5/30-125L-KQ H=45m N=22KW Q=30L/s","台",1]
[66,"潜水排污泵","65QW(I)20-15-4.0Q=20m/h3 H=15m N=4KW","台",1]
[67,"喷淋增压稳压设备","XW(L)-II-1.5-45-ADL","套",1]
[68,"室外消火栓增压稳压设备","XW(L)-II-1.5-30-ADL","套",1]
[69,"干粉灭火器","MF/ABC4","具",1]
[70,"电气工程",null,null,1]
[71,"配电箱 S1","800*2000*600","台",1]
[72,"配电箱 S2","800*2000*600","台",1]
[73,"配电箱 S3","800*2000*600","台",1]
[74,"配电箱 S4","800*2000*600","台",1]
[75,"配电箱 SAL","500*600*200","台",1]
[76,"配电箱 QWB","500*600*240","台",1]
[77,"应急照明集中电源（A型）","0.1KVA    ","台",1]
[78,"安全出口灯","集中电源集中控制型消防应急标志灯(A型)/LED 1W","套",1]
[79,"LED 天棚灯","1*12W","套",1]
[80,"LED应急型节能吸顶灯","220V  24W 应急时间180min","套",1]
[81,"自带电源的应急照明灯","36V  3W 应急时间90min","套",1]
[82,"密闭三极开关","10A 250V","个",1]
[83,"密闭双极开关","10A 250V","个",1]
[84,"单联单控开关","10A 250V","个",1]
[85,"接线盒",null,"个",1]
[86,"管内穿线","NH-BV-2.5","m",1]
[87,"管内穿线","NH-BV-4.0","m",1]
[88,"钢管","Φ15","m",1]
[89,"钢管","Φ20","m",1]
[90,"电力电缆","NH-YJV-5*4","m",1]
[91,"钢管","Φ25","m",1]
[92,"电气配线","连接软电线RVS-2*1.5","m",1]
[93,"电力电缆","NH-YJV-5*6","m",1]
[94,"电力电缆","NH-YJV-4*95","m",1]
[95,"电力电缆","NH-YJV-4*50","m",1]
[96,"电力电缆","NH-YJV-4*35","m",1]
[97,"钢管","Φ100","m",1]
[98,"钢管","Φ50","m",1]
[99,"总等电位箱","见图纸","台",1]
[100,"探测器","感温火灾探测器","个",1]
[101,"紧急启停按钮",null,"个",1]
[102,"声光报警器",null,"个",1]
[103,"报警电话",null,"个",1]
[104,"气体灭火控制器","见图纸","个",1]
[105,"指示灯",null,"套",1]
[106,"火灾警铃",null,"个",1]
[107,"启止器",null,"台",1]
[108,"电磁阀",null,"个",1]
[109,"直流电源","见图纸","台",1]
[110,"报警电话",null,"个",1]
[111,"模块","输入模块","个",1]
[112,"模块","输出模块","个",1]
[113,"压力开关",null,"个",1]
[114,"电气配线","连接软电线RVS-2*1.5","m",1]
[115,"水池液位显示仪表",null,"台",1]
[116,"水池液位计传送器",null,"支",1]
[117,"电机检查接线","XBD7.5/25-100L-KQ H=75m N=37KW Q=25L/s","台",1]
[118,"电机检查接线","XBD10/60-150L-KQ  H=100m N=90KW Q=60L/s","台",1]
[119,"电机检查接线","XBD4.5/30-125L-KQ H=45m N=22KW Q=30L/s","台",1]
[120,"电机检查接线","65QW(I)20-15-4.0\nQ=20m/h3 H=15m N=4KW","台",1]
[121,"电线","NH-BYJ-4*1.5","m",1]
[122,"电线","NH-BYJ-2*4","m",1]
[123,"电线","ZR-RVVP-2*1.5","m",1]
[124,"控制电缆头","14芯以下","个",1]
[125,"电力电缆头","400mm2以下","个",1]
[126,"电力电缆头","120mm2以下","个",1]
[127,"电力电缆头","10mm2以下","个",1]
[128,"接地母线","镀锌扁钢40*4","m",1]
[129,"接地极","镀锌钢管50*2500","根",1]

{"sheet":"室外工程","index":7,"n_rows":93,"n_cols":9,"rows_kept":93,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,2],[1,3,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[1,8,2,8],[3,1,3,2],[3,3,3,4],[4,1,4,2],[4,3,4,4],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,16,2],[16,3,16,4],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,1,23,2],[23,3,23,4],[24,1,24,2],[24,3,24,4],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,1,27,2],[27,3,27,4],[28,1,28,2],[28,3,28,4],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[31,1,31,2],[31,3,31,4],[32,1,32,2],[32,3,32,4],[33,1,33,2],[33,3,33,4],[34,1,34,2],[34,3,34,4],[35,1,35,2],[35,3,35,4],[36,1,36,2],[36,3,36,4],[37,1,37,2],[37,3,37,4],[38,1,38,2],[38,3,38,4],[39,1,39,2],[39,3,39,4],[40,1,40,2],[40,3,40,4],[41,1,41,2],[41,3,41,4],[42,1,42,2],[42,3,42,4],[43,1,43,2],[43,3,43,4],[44,1,44,2],[44,3,44,4],[45,1,45,2],[45,3,45,4],[46,1,46,2],[46,3,46,4],[47,1,47,2],[47,3,47,4],[48,1,48,2],[48,3,48,4],[49,1,49,2],[49,3,49,4],[50,1,50,2],[50,3,50,4],[51,1,51,2],[51,3,51,4],[52,1,52,2],[52,3,52,4],[53,1,53,2],[53,3,53,4],[54,1,54,2],[54,3,54,4],[55,1,55,2],[55,3,55,4],[56,1,56,2],[56,3,56,4],[57,1,57,2],[57,3,57,4],[58,1,58,2],[58,3,58,4],[59,1,59,2],[59,3,59,4],[60,1,60,2],[60,3,60,4],[61,1,61,2],[61,3,61,4],[62,1,62,2],[62,3,62,4],[63,1,63,2],[63,3,63,4],[64,1,64,2],[64,3,64,4],[65,1,65,2],[65,3,65,4],[66,1,66,2],[66,3,66,4],[67,1,67,2],[67,3,67,4],[68,1,68,2],[68,3,68,4],[69,1,69,2],[69,3,69,4],[70,1,70,2],[70,3,70,4],[71,1,71,2],[71,3,71,4],[72,1,72,2],[72,3,72,4],[73,1,73,2],[73,3,73,4],[74,1,74,2],[74,3,74,4],[75,1,75,2],[75,3,75,4],[76,1,76,2],[76,3,76,4],[77,1,77,2],[77,3,77,4],[78,1,78,2],[78,3,78,4],[79,1,79,2],[79,3,79,4],[80,1,80,2],[80,3,80,4],[81,1,81,2],[81,3,81,4],[82,1,82,2],[82,3,82,4],[83,1,83,2],[83,3,83,4],[84,1,84,2],[84,3,84,4],[85,1,85,2],[85,3,85,4],[86,1,86,2],[86,3,86,4],[87,1,87,2],[87,3,87,4],[88,1,88,2],[88,3,88,4],[89,1,89,2],[89,3,89,4],[90,1,90,2],[90,3,90,4],[91,1,91,2],[91,3,91,4],[92,1,92,2],[92,3,92,4]]}
["材料明细"]
["序号","材料名称",null,"规格型号",null,"单位","数量","备注","单价"]
[]
[1,"无缝钢管 ",null,":DN38*2.5\n",null,"m",1,"除锈红丹防锈漆一遍、耐热防腐漆两遍、硬质聚氨酯管壳保温厚50mm、铝箔保护层、冷底油两遍"]
[2,"无缝钢管 ",null,"DN45*2.5\n",null,"m",1,"除锈红丹防锈漆一遍、耐热防腐漆两遍、硬质聚氨酯管壳保温厚50mm、铝箔保护层、冷底油两遍"]
[3,"无缝钢管 ",null,"DN89*3.5\n",null,"m",1,"除锈红丹防锈漆一遍、耐热防腐漆两遍、硬质聚氨酯管壳保温厚50mm、铝箔保护层、冷底油两遍"]
[4,"无缝钢管 ",null,"DN108*4\n",null,"m",1,"除锈红丹防锈漆一遍、耐热防腐漆两遍、硬质聚氨酯管壳保温厚50mm、铝箔保护层、冷底油两遍"]
[5,"采暖无缝钢管 DN133*4",null,"DN133*4\n",null,"m",1,"除锈红丹防锈漆一遍、耐热防腐漆两遍、硬质聚氨酯管壳保温厚50mm、铝箔保护层、冷底油两遍"]
[6,"蝶阀 ",null,"DN38",null,"个",1,"钢制"]
[7,"平衡阀",null,"DN38",null,"个",1,"钢制"]
[8,"蝶阀 ",null,"DN45",null,"个",1,"钢制"]
[9,"平衡阀",null,"DN45",null,"个",1,"钢制"]
[10,"蝶阀 ",null,"DN89",null,"个",1,"钢制"]
[11,"平衡阀 ",null,"DN89",null,"个",1,"钢制"]
[12,"蝶阀 ",null,"DN108",null,"个",1,"钢制"]
[13,"平衡阀",null,"DN108",null,"个",1,"钢制"]
[14,"碟阀 ",null,"DN133",null,"个",1,"钢制"]
[15,"平衡阀 ",null,"DN133",null,"个",1,"钢制"]
[16,"管道支架",null,"角钢",null,"kg",1,"除锈、刷油设计要求:手工除锈、刷红丹二遍、热沥青二遍"]
[17,"电气设备安装工程√",null,null,"标段：S10综合楼、室外工程"]
[20,"电缆",null,"5-UTP5e-4*(2*0.5)电缆\n",null,"m",1]
[21,"PSP穿线管",null,"Φ50",null,"m",1]
[22,"通信电缆",null,"HYV20-10(2*0.5)\n",null,"m",1]
[23,"射频同轴电缆",null,"SYV75-9\n",null,"m",1]
[24,"通信电缆",null,"HYV20-50(2*0.5)\n",null,"m",1]
[25,"铠装聚氯乙烯电力电缆",null," YJV22-1KV  4*150+1*70",null,"m",1]
[26,"电力电缆",null,"YJV22-4*95+1*50\n",null,"m",1]
[27,"电力电缆",null,"YJV22-1KV  4*50+1*25",null,"m",1]
[28,"电力电缆",null,"YJV22-1KV  4*70+1*35",null,"m",1]
[29,"电力电缆",null,"NH-YJV22-1KV  4*25+1*16",null,"m",1]
[30,"电力电缆",null,"NH-YJV22-1KV  4*240+1*120",null,"m",1]
[31,"电力电缆",null,"YJV22-1KV  4*25+1*16",null,"m",1]
[32,"电力电缆",null,"YJV22-1KV  4*35+1*16",null,"m",1]
[33,"PSP穿线管",null,"Φ100",null,"m",1]
[34,"电力电缆 ",null,"YJV22-1KV  5*16\n",null,"m",1]
[35,"高杆灯",null,"16*200W\n",null,"套",1,"含控制箱及配套"]
[36,"高杆灯",null,"8*200W\n",null,"套",1,"含控制箱及配套"]
[37,"高灯杆",null,"H=25米",null,"套",1,"含配套件"]
[38,"电力电缆",null,"ZR-YJV22-10KV  3*120",null,"m",1]
[39,"PSP穿线管",null,"Φ150",null,"m",1]
[40,"电力电缆",null,"ZR-YJV22-10KV  3*95\n",null,"m",1]
[41,"PSP穿线管",null,"Φ100",null,"m",1]
[42,"控制电缆",null,"NH-KVVP-10×1.5\n",null,"m",1]
[43,"PSP穿线管",null,"Φ50",null,"m",1]
[44,"消防电源线",null,"WDZN-BYJ-4\n",null,"m",1]
[45,"镀锌钢管",null,"DN25\n",null,"m",1]
[46,"消防报警线",null,"WDZN-RVS-2*1.5",null,"m",1]
[47,"镀锌钢管",null,"DN25\n",null,"m",1]
[48,"消防报警线",null,"ZR-RVVP-2*1.5\n",null,"m",1]
[49,"镀锌钢管",null,"DN25\n",null,"m",1]
[50,"多线控制线",null,"WDZN-BYJ-1.5",null,"m",1]
[51,"镀锌钢管",null,"DN25\n",null,"m",1]
[52,"消防报警线",null,"ZN-RVS-2*1.5",null,"m",1]
[53,"电气配线",null,"NH-BV-2.5",null,"m",1]
[54,"镀锌钢管",null,"DN20\n",null,"m",1]
[55,"控制电缆",null,"WDZN-KVV-4*1.5\n",null,"m",1]
[56,"镀锌钢管",null,"DN25\n",null,"m",1]
[57,"电力电缆",null,"NH-RVVP-3*6\n",null,"m",1]
[58,"PSP穿线管",null,"Φ40",null,"m",1]
[59,"扩声系统设备",null,"柱式室外防水型音柱  4*30W",null,"台",1]
[60,"电力电缆 ",null,"YJV22-1KV  5*10\n",null,"m",1]
[61,"4芯光缆",null,"1.名称、规格：4芯光缆",null,"m",1]
[62,"8芯光缆",null,"1.名称、规格：8芯光缆",null,"m",1]
[63,"硅芯管",null,"1.名称、规格：硅芯管DN40*3.5",null,"m",1]
[64,"监控摄像设备",null,"室外带红外线高清防水高速球摄像机\n",null,"台",1,"1.名称：室外带红外线高清防水高速球摄像机\n2.含稳压电源、基础、柱、线缆及浪涌保护器等辅材"]
[65,"监控摄像设备",null,"室外带红外线高清防水高速球摄像机\n",null,"台",1,"1.名称：18m高室外带红外线高清防水高速球摄像机\n2.含稳压电源、基础、柱、线缆及浪涌保护器等辅材"]
[66,"配电箱",null,"监控机箱",null,"台",1]
[67,"视频编码器",null,"视频编码器",null,"架",1]
[68,"LED路灯及灯杆",null,"1*120W，金属、高10米",null,"套",1,"型号:1*120W，灯杆材质及高度:金属、高10米，灯杆形式（单、双）:单"]
[69,"LED庭院灯及灯杆",null,"1*40W，高3.5米\n",null,"套",1,"LED太阳能庭院灯，型号:1*40W，灯杆材质及高度:金属、高3.5米，灯杆形式（单、双）:单"]
[70,"水电桩",null,"水电桩用电负荷约为5～7KW(包括水电计费)",null,"套",1]
[71,"读卡器",null,"读卡器",null,"台",1]
[72,"储卡盒",null,"储卡盒",null,"个",1]
[73,"人(手）孔砌筑",null,"手孔井",null,"个",1]
[74,"穿刺线夹",null,"1.穿刺线夹",null,"套",1]
[75,"软件系统",null,"1.软件系统",null,"套",1]
[76,"视频管理计算机",null,"视频管理计算机",null,"台",1]
[77,"控制台",null,"控制台",null,"台",1]
[78,"安装辅材",null,"1.安装辅材",null,"套",1]
[79,"电力电缆头",null,"YJY22-4X150+1x70",null,"套",1]
[80,"电力电缆头",null,"YJV22-4x95+1x50",null,"套",1]
[81,"电力电缆头",null,"YJV22-4x50+1x25",null,"套",1]
[82,"电力电缆头",null,"YJY22-4X70+1x35",null,"套",1]
[83,"电力电缆头",null,"NH-YJY-4x25+1x16",null,"套",1]
[84,"电力电缆头",null,"NH-YJY22-4X240+1x120",null,"套",1]
[85,"电力电缆头",null,"YJY22-4x25+1x16",null,"套",1]
[86,"电力电缆头",null,"YJY22-4x35+1x16",null,"套",1]
[87,"电力电缆头",null,"YJY22-5x16",null,"套",1]
[88,"电力电缆头",null,"控制电缆",null,"套",1]
[89,"电力电缆头",null,"弱电电缆 ",null,"套",1]
[92,"商品混凝土",null,"C35",null,"m3",1]
[93,"商品混凝土",null,"C10",null,"m3",1]
[94,"铁艺围墙",{"$nulls":3},"m",1]

{"sheet":"充电桩车棚光伏","index":8,"n_rows":23,"n_cols":9,"rows_kept":23,"merged":[[0,0,0,7],[1,0,1,3],[1,4,1,7],[2,0,4,0],[2,1,4,2],[2,3,4,4],[2,5,4,5],[2,6,4,6],[2,7,4,7],[2,8,3,8],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,16,2],[16,3,16,4],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,0,23,1],[23,2,23,3],[23,4,23,7]]}
["材料明细表"]
["工程名称：充电桩车棚光伏",{"$nulls":3},"标段：s10施工图设计【光储能系统】"]
["序号","材料名称",null,"规格型号",null,"单位","数量","备注","单价"]
[]
[]
[1,"单晶硅光伏板",null,"590wp",null,"块",1]
[2,"逆变器",null,"120kw",null,"套",1,"壁挂安装"]
[3,"逆变器",null,"20kw",null,"套",1,"壁挂安装"]
[4,"逆变器",null,"17kw",null,"套",1,"壁挂安装"]
[5,"逆变器",null,"40kw",null,"套",1,"壁挂安装"]
[6,"电力电缆",null,"ZR-YJV-0.6/1KV-4*120+1*70",null,"米",1]
[7,"电力电缆",null,"ZR-YJV-0.6/1KV-5*16",null,"米",1]
[8,"电力电缆",null,"ZR-YJV-0.6/1KV-4*50+1*25",null,"米",1]
[9,"电力电缆",null,"ZR-YJV-0.6/1KV-4*26+1*16",null,"米",1]
[10,"电力电缆",null,"ZR-YJV-0.6/1KV-4*95+1*50",null,"米",1]
[11,"电缆保护管",null,"SC100",null,"米",1]
[12,"电缆保护管",null,"SC50",null,"米",1]
[13,"电缆保护管",null,"SC32",null,"米",1]
[14,"并网柜",{"$nulls":3},"套",1]
[15,"扁钢",null,"40*4",null,"米450",1]
[16,"室外储能柜",null,"215Kwh/100kw",null,"套",1]
[17,"光伏储能管理系统",null,"厂家配套",null,"套",1,"含软硬件"]
[18,"垂直风力发电机及杆件",null,"20kw/12米高",null,"套",1]

{"sheet":"充电桩","index":9,"n_rows":22,"n_cols":9,"rows_kept":22,"merged":[[0,0,0,7],[1,0,3,0],[1,1,3,2],[1,3,3,4],[1,5,3,5],[1,6,3,6],[1,7,3,7],[1,8,2,8],[4,1,4,2],[4,3,4,4],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,16,2],[16,3,16,4],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,0,22,1],[22,2,22,3],[22,4,22,7]]}
["材料明细表"]
["序号","材料名称",null,"规格型号",null,"单位","数量","备注","单价"]
[]
[]
[1,"厢式变压器",null,"1250KVA",null,"台",1]
[2,"高压柜",null,"10KV",null,"台",1]
[3,"低压柜",null,"0.4KV ",null,"台",1]
[4,"电容补偿柜",null,"0.4KV ",null,"台",1]
[5,"19\"机柜",null,"30U",null,"台",1]
[6,"无线网关",{"$nulls":3},"台",1]
[7,"多功能仪表",{"$nulls":3},"台",1,"带漏电和温度监控"]
[8,"工业交换机",{"$nulls":3},"台",1]
[9,"镀锌角钢",null,"L50*50*5",null,"米",1]
[10,"镀锌扁钢",null,"50*5",null,"米",1]
[11,"高压电缆",null,"ZC-YJV22-8.7/15-3*95",null,"米",1]
[12,"镀锌钢管",null,"DN100",null,"米",1]
[13,"镀锌钢管",null,"DN150",null,"米",1]
[14,"电力电缆",null,"ZR-YJV-0.6/1KV-4*150+1*70",null,"米",1]
[15,"电力电缆",null,"ZR-YJV-1.8/3KV-2*120+1*70",null,"米",1]
[16,"网线",null,"超5类屏蔽网线",null,"米",1]
[17,"电源线",null,"RVV2*4",null,"米",1]
[18,"镀锌钢管",null,"DN50",null,"米",1]